EE 5356 - DIGITAL IMAGE PROCESSING - PROJECT 14

Low-pass and High-pass filter

Steps:

1. Read any 512\*512 grayscale image and compute its Fourier transform.

2. Generate an ideal LPF for your 512\*512 image with cutoff frequency (Do) 40, 60 and compute its frequency response .

3. Generate a Gaussian LPF with σ = 16, 24 and compute its frequency response.

4. Generate a Butterworth LPF having order n = 3, 4 and Do = 50 and compute its frequency response.

5. Generate an ideal HPF with cutoff frequency 30, 50 and compute its frequency response.

6. Generate a Gaussian HPF with σ = 16, 24 and compute its frequency response.

7. Generate a Butterworth HPF with n = 3, 4 and Do = 50 and compute its frequency response.

8. Apply all the generated filters on your image in frequency domain and obtain the filtered images.

Submit the following:

1. Display the image and the log of its shifted Fourier transform image (magnitude spectrum).

2. Display the 3D plot of all the LPF and HPF filter responses.

3. Display all the filtered images in frequency domain.

4. Display all the filtered images in spatial domain.

5. Give the MATLAB code.

References:

1. Marques, Oge “Practical image and video processing using MATLAB” pp 243-251, Wiley, 2011